Report

Problems completed:

1. Prusa not printing
   1. Hot end case was not tightened, so head was free to spin.
2. Second Extruder was not printing
   1. Extruder was not recognising commands – Solved by downloading the config file that was set up by creatbot.
   2. Extruder direction was inverted – swapped a+ with b+ and a- with b-.

Problems still to complete:

* Second extruder is not printing supports properly
  + The hardened steel nozzle is a few mms higher than the other one. Meaning it is set off from the ground.
* LCD screen not displaying anything in python 3
* Raspberry pi shell not made
  + Designs drawn, nearly finished in cad.

Files:

<https://github.com/tunderscore2t/Kibble-Work-Experience>